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Test drive the engine and note any exhaust leakage.

Heated _s (HO28S), replacing
Heated oxygen sensors (HO2S), removing

Remove the hose between preheating and the air cleaner (ACL).
Disconnect the connectors.
Expose the wiring.

Remove the heated DXygen sensors (HO2S). Use tool 999 5543 .
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Installing heated BXygen Sensofs (HO2S)

Install the heated bXygen sensors (HO2S). Use tool 999 5543 .
Tighten to 45 Nm.

Reconnect connectors.
Secure wiring.
Install the hose between preheating and the air cleaner (ACL).





image3.png
999 5543 SOCKET NV-22 HO2S
999 5543 SOCKET NV-22 HO2S
Tool 9995
number: 7
Tool SOCk
description: NV-2:
Index HO2¢
(oxY
SENS
. Tool board: EU12
e Tool H7
position:
Tool board: SV12
Print Topic TDD.I . 7
position:
Tool board: UK2g
VOLVO o
Print Screen position:
Tool board: US12
Tool H7
position:
Help.
Suspend
Return
<l m )
T Ty Ter— . P Q@ 2o





