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Computers and Control Systems: Testing and Inspection Procedures
Extracting Diagnostic Trouble Codes

Entering Control Function #1

ACCESSING CONTROL FUNCTION #1 (fault codes)

EXTRACTING FAULT CODES:

Open the diagnostic socket cover and connect the selector cable into the appropriate socket.
a.  For fuel injection trouble shooting use socket 2 (of the 6 available).
b.  For ignition trouble shooting use socket 6 (of the 6 available).

Turn the ignition ON.
Enter control function #1 by pressing the button once for at least 1 second, but not more than 3 seconds.

Reading Light Diode
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‘Watch the light diode and count the number of flashes in the three flash series indicating a fault code. Make note of the fault codes.

If no fault codes are received by the diagnostic unit, the diode will flash 1-1-1 and the fuel injection system is O.K..

If the light diode doesn't flash when the button is depressed, or the light stays on without flashing, see DIAGNOSTIC SOCKET under

COMPONENT TESTING.





