ABSLT TPS   19.6%	ABSLT TPS  19.6%	ABSLT TPS  14.9%	ABSLT TPS 25.5  
CALC LOAD   6.3%	CALC LOAD  5.9%  	CALC LOAD 3.5%  	CALC LOAD  12.6% 
COOLANT      90 C	COOLANT    90 C	COOLANT 90 C              COOLANT 91 C	
ENG SPEED   793rpm	ENG SPEED 828    	ENG SPEED 757    	ENG SPEED  1658    
FUEL SYS 1 CLSD	FUEL SYS 1 CLSD	FUEL SYS 1 CLSD	FUEL SYS 1 CLSD	
FUEL SYS 2 CLSD	FUEL SYS 2 CLSD	FUEL SYS 2 CLSD	FUEL SYS 2 CLSD	
IAT	         68C	IAT	  69 C                 IAT	71C	            IAT 72		
IGN ADV	6	IGN ADV  -2.5	             IGN ADV  4.5               IGN ADV 38.0	
LT FTRM1   -0.8	LT FTRM1   -0.8	LT FTRM1   -0.8	LT FTRM1  -0.8 	
LT FTRM2   -0.8	LT FTRM2  -0.8 	LT FTRM2   -0.8	LT FTRM2 -0.8  	
MAF (Gr/S)  7.50	MAF (Gr/S)  6.25 	MAF (Gr/S)  7.00	MAF (Gr/S) 13.00  
MIL DIST  0 		MIL DIST    0	             MIL DIST   0 	             MIL DIST  0 	
MIL STATUS Off	MIL STAT On               MIL STAT Off                  MIL STAT Off   
O2S12	       0.000	O2S12	0.000	            O2S12	0.000	             O2S12	0.000	
02S22         0.085	02S22  0.065		02S22	0.055	             02S22	0.055	
OBD2 STAT CA		OBD2 STAT CA	             OBD2 STAT CA             OBD2 STAT CA 
ST FTRM1 32%		ST FTRM1  32%	ST FTRM1 30.5%	ST FTRM1 32.8%	
ST FTRM2 31.3	ST FTRM2  33.6%	ST FTRM2 26.6%	ST FTRM2 31.3%      
VEH SPEED 0		VEH SPEED 0	             VEH SPEED 0	            VEH SPEED 0	



LT FTRM1 -0.8 doesn’t change
LT FTRM2 -.08 doesn’t change

FUEL SYS 1 shows OPEN when engine cold
FUEL SYS 2 shows OPEN when engine cold


FUEL SYS 1 changes from CLSD to OPEN2 when engine reaches approx. 2000 RPM		
FUEL SYS 2 changes from CLSD to OPEN2 when engine reaches approx. 2000 RPM	








	

[bookmark: _GoBack]
O2 Bank 1 Sensor 1			O2 Bank 2 Sensor 1

Test      $81					Test     $81
MOD    $11					MOD   $11
MAX	255					MAX	255
MEAS	128					MEAS	124
MIN	90					MIN	90


Test	 $82					Test	$82
MOD	$11					MOD	$11
MAX	255					MAX	255
MEAS	128					MEAS	128
MIN	90					MIN	90


O2 Bank 1 Sensor 2			O2 Bank 2 Sensor 2

RICH LN Tresh					RICH LN Tresh
MOD	$11					MOD	$11
MAX	----(V)					MAX	----(V)
MEAS	0.565 (V)				MEAS	0.565 (V)
MIN	----(V)					MIN   	----(V)

LN RICH Tresh					LN RICH Tresh
MOD	$11					MOD	$11
MAX	---- (V)					MAX	---(V)
MEAS	0.565 (V)				MAX	0.565 (V)
MIN	---- (V)					MIN	----(V)
